**ARAHAN UMUM KEPADA PETENDER/PENYEBUT HARGA**

1. Petender/Penyebut harga diwajibkan mencatat pada setiap kotak pada ruangan YA/TIDAK.
2. Petender/Penyebut harga hendaklah mengisi maklumbalas di ruangan **MAKLUMBALAS PETENDER/PENYEBUT HARGA**. Kegagalan mengisi maklumbalas di ruangan berkenaan membolehkan UMT **BERHAK** untuk **TIDAK MEMPERTIMBANGKAN** segala cadangan dan tawaran daripada petender/penyebut harga.
3. Sekiranya terdapat aksesori tambahan, sila kemukakan keterangan spesifikasi yang lengkap secara berasingan dan nyatakan seperti *Lampiran*.
4. Sekiranya terdapat spesifikasi yang bertentangan dengan maklumat sebenar sama ada pada katalog ataupun alatan sebenar, pihak UMT berhak menolak tawaran tersebut.
5. Tempoh **SAH LAKU** harga yang ditawarkan hendaklah sekurang-kurangnya **90 hari** dari tarikh tutup iklan.
6. Petender/Penyebut harga tidak dibenarkan sama sekali meletakkan tanda pengenalan syarikat pada mana-mana muka surat dalam **Borang Tawaran Spesifikasi/Katalog**. Surat akuan ‘authorised dealer’ (jika ada) hendaklah dimasukkan ke dalam Borang Tawaran Spesifikasi. Kegagalan berbuat demikian boleh menyebabkan tawaran tender/sebut harga tidak akan dipertimbangkan.
7. UMT berhak menawarkan bekalan secara per item kepada petender/penyebut harga.

|  |  |
| --- | --- |
| Logo, company name  Description automatically generated | **UNIVERSITI MALAYSIA TERENGGANU****PEJABAT BENDAHARI****BORANG TAWARAN SPESIFIKASI** |

|  |
| --- |
| **UNTUK KEGUNAAN JAWATANKUASA PEMBUKA TENDER/SEBUT HARGA** |
|
| Kod Petender/Penyebut Harga: | Tandatangan 1 : |
| Tandatangan 2 :   |

|  |  |  |
| --- | --- | --- |
| TAJUK TENDER/SEBUT HARGA | : | **SEBUT HARGA MEMBEKAL, MENGHANTAR, MEMASANG, MENGUJI DAN MENUGASMULA PERALATAN MAKMAL UNTUK KEGUNAAN UNIVERSITI MALAYSIA TERENGGANU**  |
| NO. RUJUKAN | : |  |
| NO. PETI TAWARAN | : |  |
| TARIKH TUTUP | : |  |
| MASA | :  | **12.00 TENGAHARI** |
| ITEM | : | **02** |
| NAMA ITEM | : | **SIEVE SHAKER (0.063 mm - 6.3 mm)** |
| KUANTITI | : | **1 UNIT** |
| LOKASI | : | **MAKMAL BENDALIR, ARAS BAWAH, BANGUNAN FTKKI****FAKULTI TEKNOLOGI KEJURUTERAAN KELAUTAN & INFORMATIK** |
|  |  |  |
| 1. **SPESIFIKASI WAJIB AM**
 | **:-**  |
|  |  |
| **SIEVE SHAKER SPECIFICATION**  | **MAKLUMBALAS PETENDER/PENYEBUT HARGA****√ - Memenuhi Spesifikasi****× - Tidak Memenuhi Spesifikasi** |
|  | **REFERENCE DOCUMENTATIONS** |
| 1.1 | The supplier must provide operation manual for user guideline.  |

|  |
| --- |
|  |

 |  |
| 1.2  | The supplier must provide trouble shooting manual for user guideline. |

|  |
| --- |
|  |

 |  |
| 1.3 | The supplier must provide maintenance manual for user guideline. |

|  |
| --- |
|  |

 |  |
| **2** | **CATALOGUES** |
| 2.1 | The supplier must provide original catalogues that further explain the functions and operation capabilities of the equipment offered for evaluation. |

|  |
| --- |
|  |

 |  |
| **3** | **INSTALLATION, COMMISSIONING AND TRAINING** |
| 3.1  | The supplier is responsible for the delivering, installation, test and commissioning of this equipment. Any necessary or additional material for the commissioning is at supplier cost. |

|  |
| --- |
|  |

 |  |
| 3.2  | The supplier is responsible to install and test every single unit of the instrument. |

|  |
| --- |
|  |

 |  |
| 3.3  | Upon completion of the installation and commissioning, onsite training must be conducted following successful installation and commissioning. If applicable, the commissioning must include testing experiments. Lab manual and its result as reference must be provided. |

|  |
| --- |
|  |

 |  |
| 3.4  | The supplier must provide complete toolkit for general servicing, adjustment and repair of the equipment. |

|  |
| --- |
|  |

 |  |
| 3.5 | The supplier must provide operating and maintenance manual of equipment. |

|  |
| --- |
|  |

 |  |
| **4** | **EXCLUSIVITY** |
| 4.1  | The supplier must proof their exclusivity as an authorized regional distributor or dealer to supply product intended for Malaysia from the manufacturer.  |

|  |
| --- |
|  |

 |  |
| **5** | **GENUINELY** |
| 5.1 | The equipment or item delivered must be original with a production date not more than 1 year from the date of installation on site. Pirated manufactured units, unauthorized copies and clones are prohibited and not accepted. |

|  |
| --- |
|  |

 |  |
| **6** | **DELIVERY** |
| 6.1 | The product must be delivered by the supplier. UMT has the right to decline if the delivery is done using third party and without supplier's representative at site. |

|  |
| --- |
|  |

 |  |
| 6.2 | Supplier must bear the cost to provide sufficient manpower/ machineries to place the equipment in respective laboratory:* Makmal Bendalir, Aras bawah, Fakulti Teknologi Kejuruteraan Kelautan dan Informatik
 |

|  |
| --- |
|  |

 |  |
| **7** | **WARRANTY** |
| 7.1  | The supplier must provide a good sales service for all equipment supplied. |

|  |
| --- |
|  |

 |  |
| 7.2  | The supplier must provide warranty of at least/ minimum 1 year for spare parts and accessories of this equipment. |

|  |
| --- |
|  |

 |  |
| 7.3 | The supplier must provide warranty card and immediate response upon breakdown within 3 working days. |

|  |
| --- |
|  |

 |  |

|  |  |
| --- | --- |
| 1. **SPESIFIKASI WAJIB**
 | **:-**  |
|  |  |
| **SIEVE SHAKER SPECIFICATION**  | **MAKLUMBALAS PETENDER/PENYEBUT HARGA****√ - Memenuhi Spesifikasi****× - Tidak Memenuhi Spesifikasi****Nyatakan Spesifikasi Yang Ditawarkan** |
| 1 | Robust and compact laboratory mechanical test sieving machine. |

|  |
| --- |
|  |

 |  |
| 2 | Sieve diameter: 200mm, with woven wire mesh. |

|  |
| --- |
|  |

 |  |
| 3 | Maximum height of sieves stacking: at least 400mm |

|  |
| --- |
|  |

 | Your offer: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

|  |  |
| --- | --- |
| **C) SPESIFIKASI TEKNIKAL** | **:-**  |
|  |  |
| **SIEVE SHAKER SPECIFICATION**  | **MAKLUMBALAS PETENDER/PENYEBUT HARGA****√ - Memenuhi Spesifikasi****× - Tidak Memenuhi Spesifikasi****Nyatakan Spesifikasi Yang Ditawarkan** |
| 1 | Sieve drive and motion: Electromagnetic drive and 3D motion. |

|  |
| --- |
|  |

 |  |
| 2 | Maximum batch quantity: at least 2kg per sieving operation |

|  |
| --- |
|  |

 | Your offer: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 3 | Amplitude: at least 0 – 2mm, digitally adjustable. |

|  |
| --- |
|  |

 | Your offer: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

|  |  |
| --- | --- |
| **D)** | **Jenama/Model/Buatan Yang Ditawarkan** |
| **JENAMA** | **MODEL** | **BUATAN** **(NEGARA)** |
|  |  |  |

*\* Jenama/Model/Buatan yang ditawarkan MESTILAH sama seperti di Borang Tawaran Harga*